This message is a reply to CCS e-mail id: 9J7153

Attached is firmware for the ezWebLynx 5V Rev1 with LCD.  In DOS, perform this command:

tftp -i 192.168.100.210 put estamp.5v.rev1.lcd.merged.bin bootload.bin

Replace the 192.168.100.210 with the IP address of your unit.

After the file uploads, the LEDs will blink for a minute as the firmware gets written to the processor.  When the upgrade is complete, perform an AT*VER? and double check that the version is 1.015.

Regards,
Darren @ CCS
262-522-6500 x72

> Hello
>
> How can I activate the function LCD_SEND in a module 5V Rev1?
>
> Thanks
> ABI
>

