004     @WRITE_PROGRAM_MEMORY8.P1
004-005 @READ_PROGRAM_MEMORY8.P2
006     port_b
015-016 CCP_1
015     CCP_1_LOW
016     CCP_1_HIGH
01B     CCP_2_LOW
01B-01C CCP_2
01C     CCP_2_HIGH
020     @TRIS_C
021-031 MAIN.cadena
032     MAIN.letra
033     MAIN.i
034     LCD_INI.num
034     LCD_GOTOXY.x
034     MAIN.@SCRATCH1
035     @delay_ms1.P1
035     LCD_GOTOXY.y
035     MAIN.@SCRATCH2
036     LCD_GOTOXY.dir
036     LCD_DATO.datod
037     LCD_GOTOXY.@SCRATCH1
038     LCD_INSTR.datoi
039     LCD_BUSY.data
077     @SCRATCH
078     @SCRATCH
078     _RETURN_
079     @SCRATCH
07A     @SCRATCH
07B     @SCRATCH
09C.6   C1OUT
09C.7   C2OUT
10D-10E @WRITE_PROGRAM_MEMORY8.P1
10D-10E @READ_PROGRAM_MEMORY8.P2

ROM Allocation:
00A2  @delay_ms1
008B  LCD_E
0067  LCD_BUSY
0095  LCD_INSTR
00D9  LCD_DATO
00E6  LCD_GOTOXY
00B7  LCD_INI
00F6  MAIN
0004  @const74
0017  @const75
0032  @const77
00F6  @cinit

Project Directory:
    C:\ezweb\ejer15\programa_pic\

Project Files:
    project15.c
    ..\..\..\ARCHIV~1\PICC\devices\16F876A.h
    lcd.h

Units:
    project15.c (main)

Compiler Settings:
    Processor:      PIC16F876A
    Pointer Size:   16
    ADC Range:      0-255
    Opt Level:      9
    Short,Int,Long: UNSIGNED: 1,8,16
    Float,Double:   32,32

Output Files:
    Errors:      project15.err
    Ext Symbols: project15.esym
    INHX8:       project15.hex
    Symbols:     project15.sym
    List:        project15.lst
    Debug/COFF:  project15.cof
    Project:     project15.PJT
    Call Tree:   project15.tre
